SFML 2.3.2

- Main Page
- Related Pages
- Modules
- Classes
- Files

- File List

Sensor.hpp
1 //
3 // SFML - Simple and Fast Multimedia Library
4 // Copyright (C) 2007-2015 Laurent Gomila (laurent@sfml-dev.org)
5 //
6 // This software is provided 'as-is', without any express or implied warranty.
7 // In no event will the authors be held liable for any damages arising from the use of this software.
8 //
9 // Permission is granted to anyone to use this software for any purpose,
10 // including commercial applications, and to alter it and redistribute it freely,
11 // subject to the following restrictions:
12 //
13 // 1. The origin of this software must not be misrepresented;
14 // you must not claim that you wrote the original software.
15 // If you use this software in a product, an acknowledgment
16 // in the product documentation would be appreciated but is not required.
17 //
18 // 2. Altered source versions must be plainly marked as such,
19 // and must not be misrepresented as being the original software.
20 //
21 // 3. This notice may not be removed or altered from any source distribution.
22 //
24
25 #ifndef SFML_SENSOR_HPP
26 #define SFML_SENSOR_HPP
27
29 // Headers
31 #include <SFML/Window/Export.hpp>
32 #include <SFML/System/Vector3.hpp>
33 #include <SFML/System/Time.hpp>
34
35
36 namespace sf
37 {
42 class SFML_WINDOW_API Sensor
43 {
44 public:
45
50 enum Type
51 {
52 Accelerometer,
53 Gyroscope,
54 Magnetometer,
55 Gravity,
56 UserAcceleration,
57 Orientation,
58
59 Count
60 };
61
70 static bool isAvailable(Type sensor);
71
85 static void setEnabled(Type sensor, bool enabled);
86
95 static Vector3f getValue(Type sensor);
96 };
97
98 } // namespace sf
99
100
101 #endif // SFML_SENSOR_HPP
102
103
sf::Sensor
Give access to the real-time state of the sensors.
Definition: Sensor.hpp:42
sf::Sensor::Accelerometer
Measures the raw acceleration (m/s^2)
Definition: Sensor.hpp:52
sf::Sensor::Type
Type
Sensor type.
Definition: Sensor.hpp:50
sf::Vector3
Utility template class for manipulating 3-dimensional vectors.
Definition: Vector3.hpp:37
sf::Sensor::UserAcceleration
Measures the direction and intensity of device acceleration, independent of the gravity (m/s^2) ...
Definition: Sensor.hpp:56
sf::Sensor::Gyroscope
Measures the raw rotation rates (degrees/s)
Definition: Sensor.hpp:53
sf::Sensor::Magnetometer
Measures the ambient magnetic field (micro-teslas)
Definition: Sensor.hpp:54
sf
Definition: AlResource.hpp:34
sf::Sensor::Orientation
Measures the absolute 3D orientation (degrees)
Definition: Sensor.hpp:57
sf::Sensor::Gravity
Measures the direction and intensity of gravity, independent of device acceleration (m/s^2) ...
Definition: Sensor.hpp:55